How to perform a firmware update?

Method: Firmware upgrade via USB

1. Download the latest firmware from the support section for each product/product page. 
2. Format the USB drive to FAT16/FAT32.
3. Store the uncompressed firmware filed onto the root directory of the USB drive.
4. Connect the USB drive with the firmware to the desired light fixture via the USB port
found on the control box.
5. Enter the system menu and select "Firmware Update" and select "Start" to intiate the update.

Method: Firmware upgrade via Sidus Link OTA

1. Connect the light fixture to your Sidus Link Smart Device.
1a. Perform a Bluetooth (BT Reset) on your fixture.
1b. In your Sidus Link Scene tap on the green (+) symbol and then tap on "New Fixtures."
2. Locate the fixture you would like to update and tap on the "⋮" symbol.
3. If there is a firmware update available for your fixture there will be an orange dot displayed
next to "Firmware Update." If there is an update available, tap on "Firmware Update," to initiate
the upgrade.