How to perform a firmware update?

Method: Firmware upgrade via USB

1. Download the latest firmware from the support section for each product/product page. 
2. Format the USB drive to FAT16/FAT32.
3. Store the uncompressed firmware filed onto the root directory of the USB drive.
4. Connect the USB drive with the firmware to the desired light fixture via the USB port
found on the control box.
5. Enter the system menu and select "Firmware Update" and select "Start" to intiate the update.

